SSequencer Beta BOM
========================
(version beta 1 - 2/12/2023)

1 - Arduino Due (Mega won't work!! PCB runs at 3.3volts. Mega runs at 5v and may damage components)
1 - Arduino Due compatible power supply; sometimes USB power is not enough and the displays go dim
1 - microSD Card compatible with Arduino

AMAZON
1 - 1x40 16 Pin Headers Male 2.54mm Single Row Straight Needle Connector (19mm)
	** tall headers for the LCD display to pass through PCB

1 - HiLetgo 2pcs MAX7219 8-Digital Segment Digital LED Display Tube for Arduino 51/AVR/STM32 (or similar Arduino compatible)

16 - EDGELEC 3mm Yellow Lights LED Diodes (Yellow Lens)(DC 2V)
16 - EDGELEC 3mm Red Lights LED Diodes (Red Lens)(DC 2V)
16 - EDGELEC 3mm Green Lights LED Diodes (Green Lens)(DC 3V)
	** (if you use diffent LEDs with different voltages you may need to change the 82 ohm current limiting resistors)

1 - Weewooday 8 Pieces IIC/ I2C/ TWI LCD Serial Interface Adapter and LCD Module Display 
	** Backlight Compatible with Arduino R3 MEGA2560 (Blue,LCD 1602 16 x 2)
	** I buy these because the two part boards are not soldered together which is need as the SS1 PCB goes in between them

1 - Adafruit 4682 Micro SD SPI or SDIO Card Breakout Board - 3V ONLY! 

35 - 1N4148 Switching Diode 200 mA 100 V DO-35 Axial 4148 200 milliamp 100 Volt Electronic Silicon Diodes(Pack of 125 Pieces)


EBAY - https://www.ebay.com/itm/173827599780?var=472521857632
13 - PB86-A0 White (no LED)
 5 - PB86-A0 Grey (no LED)
 2 - PB86-A0 Yellow (no LED)
 1 - PB86-A0 Red (no LED)
 1 - PB86-A0 Black (no LED)
 5 - PB86-A1 Blue (with LED)
 3 - PB86-A1 Green (with LED)
 4 - PB86-A1 Red (with LED)

TAYDA ELECTRONICS
5 - PJ-3001F 3.5mm Mono Phone Jack 
	** (first time I've used these and they seem a bit flakey. You might want to check metal tab connection to jack before soldering)
1 - 2N3904 NPN General Purpose Transistor
1 - 74HC125 HD74HC125P 74125 Quad Bus Buffer Tri-State IC
2 - H11L1 H11L1M High Speed Optocoupler Logic Output 1 Channel
4 - 5 Pin MIDI Connector Female Right Angle
2 - 33 Ohm 1/8W 1% Metal Film Resistor
2 - 220 Ohm 1/8W 1% Metal Film Resistor Royal OHM Top Quality
2 - 10 Ohm 1/8W 1% Metal Film Resistor Royal OHM Top Quality
2 - 470 Ohm 1/8W 1% Metal Film Resistor Royal OHM Top Quality
4 - 1K OHM 1/4W 1% Metal Film Resistor Royal OHM Top Quality
2 - 10K OHM 1/4W 1% Metal Film Resistor Royal OHM Top Quality
8 - 82 OHM 1/4W 1% Metal Film Resistor Royal OHM
1 - 2x40 Pin 2.54mm Double Row Pin Header Strip
2 - 40 Pin 2.54mm Single Row Pin Header Strip
1 - 2x4 Pin 2.54mm Double Row Female Pin Header
1 - PIEZO ELECTRONIC TONE BUZZER ALARM 30V 4000Hz PCB 2 Pins

MOUSER
1 - Bourns Encoder PEC11R-4230K-S0024 https://www.mouser.com/ProductDetail/652-PEC11R4230KS0024
